@book{Kraml,
address = {Basel},
author = {Kraml, M and Dubue, J and Gaudry, R},
editor = {Gsell, O},
isbn = {978-3-8055-0475-1},
keywords = {griseofulvin},
mendeley-tags = {griseofulvin},
pages = {232},
publisher = {Krager},
title = {{Antibiotics and Chemotherapy}},
year = {1962}
}
@article{Blaey,
author = {de Blaey, C J and Polderman, J},
issn = {0031-6911},
journal = {Pharmaceutisch weekblad},
keywords = {Drug Compounding,Tablets},
month = feb,
number = {9},
pages = {241--50},
pmid = {5415900},
title = {{Compression of pharmaceuticals. I. The quantitative interpretation of force-displacement curves.}},
url = {http://www.ncbi.nlm.nih.gov/pubmed/5415900},
volume = {105},
year = {1970}
}
@article{EMC,
author = {Callahan, J C and Cleary, G W and Elefant, M and Kaplan, G and Kensler, T and Nash, R A},
doi = {10.3109/03639048209022105},
journal = {Drug Development and Industrial Pharmacy},
number = {3},
pages = {355--369},
title = {{Equilibrium Moisture Content of Pharmaceutical Excipients}},
url = {http://informahealthcare.com/doi/abs/10.3109/03639048209022105},
volume = {8},
year = {1982}
}
@article{Lees63,
author = {Lees, K A},
journal = {J. Pharm. Pharmacol.},
pages = {43--55},
title = {{Fine particles in pharmaceutical practice. Clinical and pharmaceutical aspects}},
url = {http://www.ncbi.nlm.nih.gov/pubmed/14101625},
volume = {15},
year = {1963}
}
@article{Artega1990,
author = {Artega, P. and T\"{u}z\"{u}n, U.},
doi = {10.1016/0009-2509(90)87093-8},
issn = {00092509},
journal = {Chemical Engineering Science},
month = jan,
number = {1},
pages = {205--223},
title = {{Flow of binary mixtures of equal-density granules in hoppers—size segregation, flowing density and discharge rates}},
url = {http://linkinghub.elsevier.com/retrieve/pii/0009250990870938},
volume = {45},
year = {1990}
}
@article{Rippie,
author = {Rippie, E G and Chou, C H},
doi = {10.1016/0032-5910(78)80090-4},
issn = {0032-5910},
journal = {Powder Technology},
number = {2},
pages = {205--216},
title = {{Kinetics of mass transport in sheared particulate beds: Markov chains}},
url = {http://www.sciencedirect.com/science/article/pii/0032591078800904},
volume = {21},
year = {1978}
}
@article{lognorm,
author = {Limpert, Eckhard and Stahel, Werner A. and Abbt, Markus},
doi = {10.1641/0006-3568(2001)051[0341:LNDATS]2.0.CO;2},
file = {:home/dario/Documenti/Mendeley Desktop/2001/Limpert, Stahel, Abbt - Log-normal Distributions across the Sciences Keys and Clues.pdf:pdf},
issn = {0006-3568},
journal = {BioScience},
number = {5},
pages = {341},
title = {{Log-normal Distributions across the Sciences: Keys and Clues}},
url = {http://www.jstor.org/stable/10.1641/0006-3568\%282001\%29051\%5B0341\%3ALNDATS\%5D2.0.CO\%3B2},
volume = {51},
year = {2001}
}
@book{dallavalle1948,
author = {DallaValle, J M},
publisher = {Pitman Pub. Corp.},
title = {{Micromeritics: the technology of fine particles}},
url = {http://books.google.it/books?id=k2oaAAAAMAAJ},
year = {1948}
}
@phdthesis{Westerhuis1997,
author = {Westerhuis, Johannes Arnold},
file = {:home/dario/Documenti/Mendeley Desktop/1997/Westerhuis - Multivariate statistical modelling of the pharmaceutical process of wet granulation and tableting.pdf:pdf},
isbn = {9036707978},
pages = {157},
school = {Universit\`{a} di Groningen},
title = {{Multivariate statistical modelling of the pharmaceutical process of wet granulation and tableting}},
url = {http://irs.ub.rug.nl/ppn/16190985X},
year = {1997}
}
@article{Aerosol,
author = {Kanig, Joseph L},
doi = {10.1002/jps.2600520603},
issn = {1520-6017},
journal = {Journal of Pharmaceutical Sciences},
number = {6},
pages = {513--535},
publisher = {Wiley Subscription Services, Inc., A Wiley Company},
title = {{Pharmaceutical aerosols}},
url = {http://dx.doi.org/10.1002/jps.2600520603},
volume = {52},
year = {1963}
}
@article{EMC2,
author = {Scott, Morton W and Lieberman, Herbert A and Chow, Frank S},
doi = {10.1002/jps.2600521018},
issn = {1520-6017},
journal = {Journal of Pharmaceutical Sciences},
number = {10},
pages = {994--998},
publisher = {Wiley Subscription Services, Inc., A Wiley Company},
title = {{Pharmaceutical applications of the concept of equilibrium moisture contents}},
url = {http://dx.doi.org/10.1002/jps.2600521018},
volume = {52},
year = {1963}
}
@article{acquaCD,
abstract = {The binding capacities of ⨿-cyclodextrin samples containing different amounts of water have been investigated. Crushing strength of tablets obtained with a single-punch tableting machine was used as a measure of the cohesive properties of powders. The results clearly indicate a determinant role of adsorbed water on powder compactability. The effect of aging is also stressed and discussed.},
author = {Giordano, F and Gazzaniga, A and Bettinetti, G.P. and {La Manna}, A.},
doi = {10.1016/0378-5173(90)90229-W},
issn = {03785173},
journal = {International Journal of Pharmaceutics},
keywords = {Binding properties,Compaction,Crushing strength,Cyclodextrin,Moisture,Tablets,Water adsorption,Water desorption,$\beta$-},
month = jul,
number = {2-3},
pages = {153--156},
title = {{The influence of water content on the binding capacity of $\beta$-cyclodextrin}},
url = {http://www.sciencedirect.com/science/article/pii/037851739090229W http://linkinghub.elsevier.com/retrieve/pii/037851739090229W},
volume = {62},
year = {1990}
}
@article{Nelson,
abstract = {Energy expended in the tablet compression process was calculated by consideration of the magnitude and relation between the several compression variables. In the compression of about 0.4 Gm. of unlubricated sulfathiazole granulation to a maximum force of 1200 Kg, on the lower punch with flat-faced 3/8-inch punches, about 8.6 calories were expended. For about the same weight of lubricated granulation the corresponding value was about 2.0 calories. By considering that only energy expended in the process of eliminating void space to form the tablet caused a temperature rise in the tablet, the temperature rise expected in the lubricated or unlubricated tablets mentioned above would be about 5°. When the energies expended in the processes of tablet ejection, overcoming wall friction and removing the upper punch from the die, were summed for a single punch machine making these tablets at the rate of 100 per minute, it was found that 43 kilocalories would be expended in each hour of operation if the tablets were unlubricated. If lubricated granulation were used the value would be 3 kilocalories. The bulk of these expenditures would probably cause heating of the punches and die and if the granulation was either poorly lubricated or unlubricated the heating might be severe.},
author = {Nelson, Eino and Busse, L W and Higuchi, Takeru},
doi = {10.1002/jps.3030440413},
issn = {00959553},
journal = {Journal of the American Pharmaceutical Association},
month = sep,
number = {4},
pages = {223--225},
publisher = {Wiley Subscription Services, Inc., A Wiley Company},
title = {{The physics of tablet compression. VII. Determination of energy expenditure in the tablet compression process}},
url = {http://dx.doi.org/10.1002/jps.3030440413 http://doi.wiley.com/10.1002/jps.3030440413},
volume = {44},
year = {2006}
}
@book{Lachman,
author = {Lachman, Leon and Lieberman, Herbert A},
edition = {Special In},
isbn = {9788123916798},
pages = {902},
publisher = {CBS},
title = {{The Theory and Practice of Industrial Pharmacy}},
year = {2009}
}
